**Tender Form–Works**

|  |
| --- |
| **Title of the tender: Establishing and marking of walking trail**  **Reference number:** HUSRB/1602/31/0128/Municipality of Novi Becej/TD8 |

1. **TENDERER’S INFORMATION**

|  |  |
| --- | --- |
| Submitted by: | Name(s) and address(es) of legal entity or entities submitting this tender |
| Tenderer |  |
| Legal representative |  |
| VAT/registration number[[1]](#footnote-2) |  |
| Nationality |  |
| Address |  |
| Telephone/e-mail |  |
| Contact person |  |
| Bank data | Bank account holder name:  Bank account number:  Bank name:  SWIFT Code:  IBAN: |

1. **TENDERER’S STATEMENT**

I undersigned hereby confirm that the construction works offered in this tender are in full conformity with the specifications submitted to us by the contracting authority. The detailed description of the offered construction works by us is provided in the next point.

In addition to that we confirm that our organisation/company is fully eligible for providing construction works under a contract financed by the EU funds. We confirm that we are not in any of the situations that would exclude us from competing in the EU financed tenders as indicated in the point 2.3.3. in the PRAG Manual.

Furthermore we agree to abide by the ethics clauses in Section 2.4.14 of the PRAG Manual.

1. **TECHNICAL AND FINANCIAL OFFER**

The tenderers are required to provide technical offer, based on the requirements indicated by the contracting authority in the Instructions to Tenderers, Point 2: Technical information.

The tenderers are encouraged to provide details on the planned works, including detailed specifications and/or brand names.

* 1. **Description of works:** (Tenderers offer/response to the CA requirements)
  2. **Designs and drawings**: (Tenderer’s comments to drawings, approach and application in execution of works)
  3. **Inputs required from the tenderer**: (Tenderers offer of equipment, labour, tools, vehicles etc. as response to the CA’s requirements)

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **No.** | **Number of items** | **Title of item** | **Technical offer**  **items offered by the tenderer, based on the requirements in Point 2 of Instruction to tenderers** | **Financial offer** | |
| **Price per item without VAT [EUR] or [RSD]**  \*- Please delete currency not used for offer | **Price total**  **without VAT [EUR] or [RSD]**  \*- Please delete currency not used for offer |
| *1.1.* | *25,00* | *m²* | *Cleaning and planning terrain of shrubbery by excavator and pulling away to distance of 100m* |  |  |
| *1.2.* | *1,20* | *m³* | *Manual dig of III class soil for spot footing with proper cutting of the edges and transferring and planning the soil in the surrounding terrain. Transfer of soil to distance up to 50m¹* |  |  |
| *1.3.* | *1,50* | *m²* | *Planning of subbase with accuracy of ± 2 cm* |  |  |
| *1.4* | *1,50* | *m²* | *Procurement/provision transport and installation of natural gravel thk.= 20 cm with compaction of the the same by plate vibrator to the required compaction.* |  |  |
| *1.5* | *1,00* | *m³* | *Production of concrete foundations type MB-20.*  *Concrete work over spreaded gravel layer thickness of 20 cm.*  *Concrete should be installed and maintained according to regulations.* |  |  |
| *1.6* | *6* | *pcs.* | *Production and installation of anchor plates from galvanized thin sheet / thk.= 2mm / for*  *fixing of wooden pillars and stay 14/14 cm to oversite concrete. Anchor plate should be done according to the details provided by the investor.* |  |  |
| *1.7* | *6* | *pcs.* | *Positioning and installation of anchor plates from the galvanized thin sheet* |  |  |
| *1.8* | *1* | *pcs.* | *Production of wooden frame 106/236 cm with dimensions of wrought cross-section 14/14cm and chamfer at cadastral lot 24192 cadastral municipality Novi Becej – division Srednja strana*  *- material for production of board is dried wood (fir tree) in wood color -natural,*  *- board should be produced according to the technical drawing,*  *- stand should be produced according to technical drawing,*  *- board should be covered with the minimum of 2 layers of colorless sadolin with wax,*  *- After mounting the Info boards, place a 120x80 aluminum panel with the contents ordered by the contracting authority/orderer printed on a protective UV foil resistant form weather influences* |  |  |
| *2.1.* | *25,00* | *m²* | *Cleaning and planning terrain of shrubbery by excavator and pulling away to distance of 100m* |  |  |
| *2.2.* | *1,20* | *m³* | *Manual dig of III class soil for spot footing with proper cutting of the edges and transferring and planning the soil in the surrounding terrain. Transfer of soil to distance up to 50m¹* |  |  |
| *2.3.* | *1,50* | *m²* | *Planning of subbase with accuracy of ± 2 cm* |  |  |
| *2.4* | *1,50* | *m²* | *Procurement/provision transport and installation of natural gravel thk.= 20 cm with compaction of the the same by plate vibrator to the required compaction.* |  |  |
| *2.5* | *1,00* | *m³* | *Production of concrete foundations type MB-20.*  *Concrete work over spreaded gravel layer thickness of 20 cm.*  *Concrete should be installed and maintained according to regulations.* |  |  |
| *2.6* | *6* | *pcs.* | *Production and installation of anchor plates from galvanized thin sheet / thk.= 2mm / for*  *fixing of wooden pillars and stay 14/14 cm to oversite concrete. Anchor plate should be done according to the details provided by the investor.* |  |  |
| *2.7* | *6* | *pcs.* | *Positioning and installation of anchor plates from the galvanized thin sheet* |  |  |
| *2.8* | *1* | *pcs.* | *Production of wooden frame 146/232 cm with dimensions of wrought cross-section 14/14cm and chamfer at cadastral lot 14651 cadastral municipality Novi Becej – division Veliko kopovo*  *- material for production of board is dried wood (fir tree) in wood color -natural,*  *- board should be produced according to the technical drawing,*  *- stand should be produced according to technical drawing,*  *- board should be covered with the minimum of 2 layers of colorless sadolin with wax,*  *- the central part of the table must rotate around its vertical axis*  *- place 2 pieces of 120x83 aluminum panels with the contents ordered by the contracting authority/orderer printed on a protective UV foil resistant form weather influences* |  |  |
| *3.1.* | *25,00* | *m²* | *Cleaning and planning terrain of shrubbery by excavator and pulling away to distance of 100m* |  |  |
| *3.2.* | *1,20* | *m³* | *Manual dig of III class soil for spot footing with proper cutting of the edges and transferring and planning the soil in the surrounding terrain. Transfer of soil to distance up to 50m¹* |  |  |
| *3.3.* | *1,50* | *m²* | *Planning of subbase with accuracy of ± 2 cm* |  |  |
| *3.4* | *1,50* | *m²* | *Procurement/provision transport and installation of natural gravel thk.= 20 cm with compaction of the the same by plate vibrator to the required compaction.* |  |  |
| *3.5* | *1,00* | *m³* | *Production of concrete foundations type MB-20.*  *Concrete work over spreaded gravel layer thickness of 20 cm.*  *Concrete should be installed and maintained according to regulations.* |  |  |
| *3.6* | *6* | *pcs.* | *Production and installation of anchor plates from galvanized thin sheet / thk.= 2mm / for*  *fixing of wooden pillars and stay 14/14 cm to oversite concrete. Anchor plate should be done according to the details provided by the investor.* |  |  |
| *3.7* | *6* | *pcs.* | *Positioning and installation of anchor plates from the galvanized thin sheet* |  |  |
| *3.8* | *1* | *pcs.* | *Production of wooden frame 146/221 cm with dimensions of wrought cross-section 14/14cm and chamfer at cadastral lot 14621 cadastral municipality Novi Becej – division Veliko kopovo*  *- material for production of board is dried wood (fir tree) in wood color -natural,*  *- board should be produced according to the technical drawing,*  *- stand should be produced according to technical drawing,*  *- board should be covered with the minimum of 2 layers* *of colorless sadolin with wax,*  *- on the upper part of the board, set aluminum panel dimension 120x80 with the contents ordered by the contracting authority/orderer printed on a protective UV foil resistant form weather influences with rotating circles diameter of (6-8 pcs.) 15-18 cm with the contents ordered by the contracting authority/orderer also printed on aluminum tin with UV foil resistant form weather influences. Fix the circle at the top (in order to be able to turn around and discover the contents below the circle) but to be rotating,*  *- on the lower part of the board, relief carve wood In shape of eggs in accordance with the instructions specified by the (6-8 pcs.) and paint them with weatherproof colors according to the contracting authority/ orderer's instructions.* |  |  |
| *4.1.* | *25,00* | *m²* | *Cleaning and planning terrain of shrubbery by excavator and pulling away to distance of 100m* |  |  |
| *4.2.* | *1,20* | *m³* | *Manual dig of III class soil for spot footing with proper cutting of the edges and transferring and planning the soil in the surrounding terrain. Transfer of soil to distance up to 50m¹* |  |  |
| *4.3.* | *1,50* | *m²* | *Planning of subbase with accuracy of ± 2 cm* |  |  |
| *4.4* | *1,50* | *m²* | *Procurement/provision transport and installation of natural gravel thk.= 20 cm with compaction of the the same by plate vibrator to the required compaction.* |  |  |
| *4.5* | *1,00* | *m³* | *Production of concrete foundations type MB-20.*  *Concrete work over spreaded gravel layer thickness of 20 cm.*  *Concrete should be installed and maintained according to regulations.* |  |  |
| *4.6* | *6* | *pcs.* | *Production and installation of anchor plates from galvanized thin sheet / thk.= 2mm / for*  *fixing of wooden pillars and stay 14/14 cm to oversite concrete. Anchor plate should be done according to the details provided by the investor.* |  |  |
| *4.7* | *6* | *pcs.* | *Positioning and installation of anchor plates from the galvanized thin sheet* |  |  |
| *4.8* | *1* | *pcs.* | *Production of wooden frame 146/232 cm with dimensions of wrought cross-section 14/14cm and chamfer at cadastral lot 14651 cadastral municipality Novi Becej – division Veliko kopovo*  *- material for production of board is dried wood (fir tree) in wood color -natural,*  *- board should be produced according to the technical drawing,*  *- stand should be produced according to technical drawing,*  *- board should be covered with the minimum of 2 layers of colorless sadolin with wax,*  *-in small closet make 16 pieces of A4 format (4 in each side of the cabinet) aluminum click frames with protective pvc foil and place in them the material that will be prepared by the contracting authority/orederer. Make the material on 300 grams watercolor A4 paper.*  *- The cabinet must have a lock with a key so that it can be locked if needed.* |  |  |
| *5.1.* | *25,00* | *m²* | *Cleaning and planning terrain of shrubbery by excavator and pulling away to distance of 100m* |  |  |
| *5.2.* | *1,20* | *m³* | *Manual dig of III class soil for spot footing with proper cutting of the edges and transferring and planning the soil in the surrounding terrain. Transfer of soil to distance up to 50m¹* |  |  |
| *5.3.* | *1,50* | *m²* | *Planning of subbase with accuracy of ± 2 cm* |  |  |
| *5.4* | *1,50* | *m²* | *Procurement/provision transport and installation of natural gravel thk.= 20 cm with compaction of the the same by plate vibrator to the required compaction.* |  |  |
| *5.5* | *1,00* | *m³* | *Production of concrete foundations type MB-20.*  *Concrete work over spreaded gravel layer thickness of 20 cm.*  *Concrete should be installed and maintained according to regulations.* |  |  |
| *5.6* | *6* | *pcs.* | *Production and installation of anchor plates from galvanized thin sheet / thk.= 2mm / for*  *fixing of wooden pillars and stay 14/14 cm to oversite concrete. Anchor plate should be done according to the details provided by the investor.* |  |  |
| *5.7* | *6* | *pcs.* | *Positioning and installation of anchor plates from the galvanized thin sheet* |  |  |
| *5.8* | *1* | *pcs.* | *Production of wooden frame 146/221 cm with dimensions of wrought cross-section 14/14cm and chamfer at cadastral lot 24209 cadastral municipality Novi Becej – division Veliki pesak*  *- material for production of board is dried wood (fir tree) in wood color -natural,*  *- board should be produced according to the technical drawing,*  *- stand should be produced according to technical drawing,*  *- board should be covered with the minimum of 2 layers of colorless sadolin with wax,*  *- each of the 15x15x2cm cube must be located on the bearer and be able to rotate around the vertical axis*  *- on each cube, on both sides place an aluminum plate of the same dimensions with the content specified by the contracting authority/orderer on protective UV foil resistant form weather influences.* |  |  |
| **Financial offer – TOTAL** | | | | |  |

The offered total price for the described items indicated in the previous point is: <**XXX EUR/ RSD> total.**

**Note:**

Price must be presented in amount **excluding** all duties and taxes (e.g. VAT and all other taxes)

The offered price includes implementation/delivery of described items as well as all accompanying costs (for example transport, logistics, material costs) when required.

|  |  |
| --- | --- |
| Name of the authorised signatory |  |
| Signature |  |
| Date |  |

1. Where applicable. For individuals, mention their ID card or passport or equivalent document - number [↑](#footnote-ref-2)